                                                                   Revision: 1.0
--------------------------------------------------------------------------------
Package            update-4.0.9_4.1.1-p-4.cbsa

Version            4.1.1-p-4

Required version   4.0.9-p

Support models     Server
                   Server Advanced
                   Server 192
                   Virtual Machine

--------------------------------------------------------------------------------
WHAT THIS PACKAGE DOES

 This package updates Evolution system from version 4.0.9-p to version
 4.1.1-p-4.
 This update is generally done manually by the user following the instructions
 in the INSTALLATION section.

--------------------------------------------------------------------------------
NOTES

 Please clear your browser cache after installing this update.
 
--------------------------------------------------------------------------------
LIMITATIONS

 Nothing.

--------------------------------------------------------------------------------
CHANGES IN THIS RELEASE

[4.0.10-p]

- Improved: Implemented captive runtime installation of Editor and Connection
  Manager. Now it is not necessary to have Adobe AIR installed on the system
- Added new datapoint type dpt 29.0XX of 8 bytes.
- Implemented compativility with new Ubuntu 20.04 Evolution Systems.
- Fixed: When two scenes were saved with the same name, no error was displayed.
- Fixed: The RGBW component was sending the bytes in the wrong order.
- Fixed: Error in advanced charts with quarter hour range.
- Fixed: Error with password popup in Smartvisu.
- Fixed: Background color when edit advanced chart.
- Fixed: Error when load external link inside iframe.
- Fixed: The scene is not disabled from the scene list.
- Fixed: Scene with 6 bytes event does not work after save.
- Fixed: Is not possible to close popup in TCI touch screen with windows.
- Fixed: When the process point template has a complex name is not working.


[4.0.11-p]

- Fixed: Fixed errors in CSV export tool when export alarms log.
- Improved: Translation update system.


[4.0.12-p]

- Implemented to access the Annual Planner editor for all users from the
  Connection Manager.

[4.0.13-p]

- Fixed: The default units are correctly assigned for the water and gas
   meters
- Improved: Date and time is added in the csv export of the advanced
   charts
- Improved: Lateral gaps for advanced charts are reduced
- Improved: The long name of the meters is displayed in the smartmetering
  module tree
- Improved: Added select all button in the smartmetering tree and the
  parent folder selects all its children.
- Fixed: The rgbw element works on the smartvisu.

[4.0.14-p]

- [EVO5] - Improved: Cameras work through the apache server,
  doing a reverse proxy.
- Fix: If no language is selected, enter with the user's default language.
- Fix: Failure to activate project that occurred in 4.0.13-p

[4.0.15-p]

- Improved: In smartmetering changed select all button by root folder.
- Improved: Flag "cascade" in smartmetering tree, for enable/disable
  cascade selection.

[4.0.16-p]

- Improved: Send with the logic process points with dtp 232 and 251.
- Improved: Send with the input value element process points with
  dtp 232 and 251.
- Improved: Trigger logic, alarms and scenes with process points with
  dpt 232 and 251.
- Fix: Fixed problem duplicate telegrams when they were produced at
  the same time.
- Fix: increase_sec_on successfully initialized in database.
- Fix: Wrong calculation in the units that are not the default unit
  in the counters.
- Fix: Remove group address range validation from Client Manager.
  Sometimes the ClientManager did not take for good group addresses
  greater than 15 in the main address.

[4.1.0-p]

- Improved: Annual scheduler implemented in html.
- Fix: Limited maximum image size for editor.
- Improved: Implemented TLSv1.2 smtp authentication.
- Fix: Fixed problem when there are many CSVExport module configurations.

[4.1.1-p]

- Fix: Resolved issues from annual scheduler.
- Improvement: wse_communicator does not register process point with id = -1.
- Improvement: Possibility to connect to a gateway that it haa implemented 
version 2 of tunneling, but not in a secure way.
- Fix: The background image of the dimmer element is assigned correctly.
- Fix: Fixed communication problems with gateways with the new client manager.
- Fix: The time appears incorrectly in the advanced chart when a custom date 
range is selected.
- Fix: Importing group addresses from an ETS project sometimes failed, in 
projects that had special group addresses.

--------------------------------------------------------------------------------
INSTALLATION

[EVO5 Systems]

  1. Open a web navigator
  2. Enter the address http://<device_IP>/webmin or http://evo5/webmin
  3. Enter the user and password. If the username and password are not known,
     check the product manual or contact with Futurasmus.
  4. In the side menu, navigate to "Others" -> "Custom commands".
  5. Press the button next to "Evolution Package to upload" and search the
     update package file.
  6. Press the "Evolution Package Installer" button. Installation will begin.
     - The installation process can take several minutes. Do not close the
       browser tab or your Evolution system until you have finished.
     - If the system does not have the required previous version installed,
       the installation will be canceled.
     - If the system does not meet the conditions in the LIMITATIONS section,
       the following message will appear and the installation will be canceled.

       ***************************************************
       **                                               **
       **                                               **
       **       YOUR HARDWARE IS NOT COMPATIBLE!        **
       **                                               **
       **                                               **
       ***************************************************

  7. When the installation process is complete, it will display the result.
  8. In the side menu, navigate to "System" -> "Bootup and Shutdown".
  9. At the bottom of the page that opens, press the "Reboot System" button.
 10. Press "Reboot System" button again. The system will restart.

[Other systems]

 1. Open a web navigator
 2. Enter the address http://<device_IP>:8181/upload.php
 3. Enter the user and password. If the username and password are not known,
    check the product manual or contact with Futurasmus.
 4. Press "Select file" button and search the update package file.
 5. Press "INSTALL" button. Installation will begin.
    - The installation process can take several minutes. Do not close the
      browser tab or your Evolution system until you have finished.
    - If the system does not have the required previous version installed,
      the installation will be canceled.
    - If the system does not meet the conditions in the LIMITATIONS section,
      the following message will appear and the installation will be canceled.

      ***************************************************
      **                                               **
      **                                               **
      **       YOUR HARDWARE IS NOT COMPATIBLE!        **
      **                                               **
      **                                               **
      ***************************************************

 6. When the installation process is complete, it will display the result in
    the text field of the web page. After a few seconds the system will
    restart.

