GS2-DST decoupling relay

Decoupling/isolating relay for parallel operation of 2 motors as a group. Without mains power supply. Plug housing STAK3/STAS3. 
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. 230 V AC outputs loadable up to max. 4 A / 230 V AC in total.
Dimensions 149 x 72 x 29 (W x H x D in mm).

Fabrikat: Elsner Elektronik (www.elsner-elektronik.de)
Typ: 60560 GS2-DST

WGGS-2 decoupling relay

Decoupling/isolating relay for parallel operation of 2 motors as a group. Without mains power supply. For mounting in junction box, with motor connection terminals.  
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Total drive output max. 500 W. 
Dimensions 47 x 30 x 38 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 2032 WGGS-2

WGGS-2-AP decoupling relay 

Decoupling/isolating relay for parallel operation of 2 motors as a group. Without mains power supply. With housing, with motor connection terminals. 
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Total drive output max. 500 W. 
Dimensions 89 x 53 x 89 (W x H x D, mm, without attachments).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 2035 WGGS-2-AP

WGGS-2-APK decoupling relay 

Decoupling/isolating relay for parallel operation of 2 motors as a group. Without mains power supply. With housing and motor connection leads (input with STAS3 plug, outputs with STAK3 couplings). 
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Total drive output max. 500 W. 
Housing dimensions 89 x 53 x 89 (W x H x D, mm, without attachments).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 2036 WGGS-2-APK

WGGS-2-H decoupling relay

Decoupling/isolating relay for parallel operation of 2 motors as a group. Without mains power supply. For series installation on mounting rail, with motor connection terminals.
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Maximum 500 W per 230 V AC output.
Dimensions 53 x 90 x 50 (W x H x D in mm), 3 U

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 2037 WGGS-2-H

WGGS-4-H decoupling relay

Decoupling/isolating relay for parallel operation of 4 motors as a group. Without mains power supply. For series installation on mounting rail, with motor connection terminals.
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Maximum 500 W per 230 V AC output.
Dimensions 88 x 90 x 50 (W x H x D in mm), 5 U

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 2034 WGGS-4-H

WGGS-4 decoupling relay

Decoupling/isolating relay for parallel operation of 4 motors as a group. Without mains power supply. With housing, with motor connection terminals. 
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Total power of the 230 V drives max. 500 W.
Dimensions 160 x 80 x 57 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 203 WGGS-4

WG-N-GS-4 decoupling relay

Decoupling/isolating relay for parallel operation of 4 motors as a group. With mains power supply. With housing, with motor connection terminals. 
Operating voltage 230 V AC / 50 Hz. Control input "Up/Down" 230 V AC. Each 2 230 V outputs are protected by a 6.3 A T microfuse. Total output max. 1.5 kW, power from one output max. 600 W. 
Dimensions 160 x 80 x 57 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 202 WG-N-GS-4