KNX S4-B10 230 V actuator invitation to tender

Actuator for the KNX bus system. 4 multi-function outputs, each for 1 drive (Up/Down) or 2 switchable devices (On/Off). 10 binary inputs (actuator or bus keys). Drive runtime measurement (position feedback). Storage of a movement position, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks and priority stipulations. 
Outputs: 4 x Up/Down (8 x On/Off), 230 V AC.
Inputs: 10 x binary, variable voltage 6...80 V DC and 6...240 V AC.
535 communication objects.
Rail-mounted device (6 division units) with 4 key pairs and status LEDs. Dimensions 107 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S4-B10 230 V

KNX S2-B6 230 V actuator invitation to tender

Actuator for the KNX bus system. 2 multi-function outputs, each for 1 drive (Up/Down) or 2 switchable devices (On/Off). 6 binary inputs (actuator or bus keys). Drive runtime measurement (position feedback). Storage of a movement position, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks and priority stipulations. 
Outputs: 2 x Up/Down (4 x On/Off), 230 V AC.
Inputs: 6 x binary, variable voltage 6...80 V DC and 6...240 V AC.
277 communication objects.
Rail-mounted device (6 division units) with 2 key pairs and status LEDs. Dimensions 107 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S2-B6 230 V

KNX S1-B2 230 V actuator invitation to tender

Actuator for the KNX bus system. 1 multi-function output for 1 drive (Up/Down) or 2 switchable devices (On/Off). 2 binary inputs (actuator or bus keys). Drive runtime measurement (position feedback). Storage of a movement position, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks and priority stipulations. 
Output: 1 x Up/Down (2 x On/Off), 230 V AC.
Inputs: 2 x binary, variable voltage 6...80 V DC and 6...240 V AC.
130 communication objects.
Rail-mounted device (3 division units) with 1 key pair and status LED. Dimensions 53 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S1-B2 230 V