Sewi KNX AQS/TH-D L-Pr Presence and Room Climate Sensor invitation to tender

Combined indoor sensor for the KNX bus system. Detection of brightness (with night recognition), movement, CO2, temperature, air humidity (relative/absolute) and air pressure. Operating voltage KNX bus voltage.
Application with presence detection configuration (master/slave), 4 brightness threshold values, light control, 4 temperature threshold values, temperature PI control, summer compensation, 4 humidity threshold values, humidity PI control, dew point calculation, monitoring of the comfort field, 4 air pressure threshold values, 4 CO2 threshold values, CO2 PI control, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 449 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70399 Sewi KNX AQS/TH-D L-Pr

Sewi KNX TH L-Pr Presence and Room Climate Sensor invitation to tender

Combined indoor sensor for the KNX bus system. Detection of brightness (with night recognition), movement, temperature and air humidity (relative/absolute). Operating voltage KNX bus voltage.
Application with presence detection configuration (master/slave), 4 brightness threshold values, light control, 4 temperature threshold values, temperature PI control, summer compensation, 4 humidity threshold values, humidity PI control, dew point calculation, monitoring of the comfort field, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 377 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70398 Sewi KNX TH L-Pr

Sewi KNX AQS/TH-D Room Climate Sensor invitation to tender

Combined indoor sensor for the KNX bus system. Detection of CO2, temperature, air humidity (relative/absolute) and air pressure. Operating voltage KNX bus voltage.
Application with 4 temperature threshold values, temperature PI control, summer compensation, 4 humidity threshold values, humidity PI control, dew point calculation, monitoring of the comfort field, 4 air pressure threshold values, 4 CO2 threshold values, CO2 PI control, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 363 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70397 Sewi KNX AQS/TH-D

Sewi KNX L-Pr Presence and Brightness Sensor invitation to tender

Combined indoor sensor for the KNX bus system. Detection of brightness (with night recognition) and movement. Operating voltage KNX bus voltage.
Application with presence detection configuration (master/slave), 4 brightness threshold values, light control, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 230 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70396 Sewi KNX L-Pr

Sewi KNX L Brightness Sensor invitation to tender

Indoor brightness sensor for the KNX bus system with night recognition. Operating voltage KNX bus voltage.
Application with 4 brightness threshold values, light control, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 189 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70395 Sewi KNX L

Sewi KNX AQS Air Quality Sensor invitation to tender

Indoor CO2 sensor for the KNX bus system. Operating voltage KNX bus voltage.
Application with 4 CO2 threshold values, CO2 PI control, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 210 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70394 Sewi KNX AQS

Sewi KNX TH Temperature and Humidity Sensor invitation to tender

Combined indoor sensor for the KNX bus system. Detection of temperature and air humidity (relative/absolute). Operating voltage KNX bus voltage.
Application with 4 temperature threshold values, temperature PI control, summer compensation, 4 humidity threshold values, humidity PI control, dew point calculation, monitoring of the comfort field, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 291 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70393 Sewi KNX TH

Sewi KNX T Temperature Sensor invitation to tender

Indoor temperature sensor for the KNX bus system. Operating voltage KNX bus voltage.
Application with 4 temperature threshold values, temperature PI control, summer compensation, 4 actuating variable comparators, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 237 communication objects. 
For wall or ceiling mounting. Dimensions; diameter 105 mm, height 32 mm.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70392 Sewi KNX T