KNX S1R-B4-UP 24 V actuator invitation to tender

Actuator for the KNX bus system. 1 multi-function output for 1 drive (Up/Down). 4 inputs for binary contact or temperature sensor. Drive runtime measurement (position feedback). Storage of a movement position, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks and priority stipulations. Application with 4 temperature threshold values, 4 AND logic gates and 4 OR logic gates.
Output: 1 x Up/Down, free of potential with polarity change for a 12/24 V DC drive.
Inputs: 4 x analogue/digital.
239 communication objects.
Assembly in built-in socket. Dimensions 50 x 50 x 54 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S1R-B4-UP 24 V