Tender specifications Wireless control set Solexa II

Automatic control for shades (awnings, shutters, blinds), windows, lighting and heating. Set consisting of a control unit and weather station. Battery-operated operating unit with touch display and integrated indoor temperature sensor, with wall bracket. Weather station with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver and a 230 V drive output for shading or window. Wireless connection between the weather station and operating unit. Wireless communication with up to 16 Elsner RF actuators, 3 further Solexa II displays and 32 Elsner RF operating devices/sensors. 
Control unit dimensions 107 x 112 x 14 (W x H x D in mm), weather station dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: Solexa II set

Tender specifications operating unit Solexa II

Operating unit for Solexa II radio control system. Battery-operated with touch display and integrated indoor temperature sensor, with wall bracket. 
Dimensions 107 x 112 x 14 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: Solexa II display