SO250-UI Modbus Tank Sensor invitation to tender

Tank sensor for recording the liquid level in tanks and for distance measurement. Consisting of an evaluation unit and an ultrasonic measuring sensor. Evaluation unit with display and keypad (level/distance display, measurement setting). Interfaces: Modbus, voltage 0…10 V, current 0…20 mA, 2 additional output relays. Auxiliary voltage 230 V.
Media-resistant measuring sensor for water and heating oil, measuring range 12…250 cm.
Dimensions: Evaluation unit for rail mounting (7 width units), 123 x 89 x 61 (W x H x D in mm). Sensor diameter approx. 60 mm, height approx. 45 mm, thread 1½ inches, cable length 10 m.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70152 SO250-UI Modbus