KNX S2 actuator invitation to tender

Actuator for the KNX bus system. 2 drive outputs. Drive runtime measurement (position feedback). Storage of movement positions, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks, priority stipulations, short time and movement restrictions.
Outputs: 2 x Up/Down, free of potential, max. 30 V DC or 230 V AC.
Operating Voltage Bus Voltage.
207 communication objects.
Rail-mounted device (3 division units) with 2 key pairs and status LED. Dimensions 53 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S2

KNX S4 actuator invitation to tender

Actuator for the KNX bus system. 4 drive outputs. Drive runtime measurement (position feedback). Storage of movement positions, 16-channel scene memory.
External or internal setting of the automatic functions possible. Internal automatic functions with shading or window control, blocks, locks, priority stipulations, short time and movement restrictions.
Outputs: 4 x Up/Down, free of potential, max. 30 V DC or 230 V AC.
Operating Voltage 230 V AC.
409 communication objects.
Rail-mounted device (6 division units) with 4 key pairs and status LEDs. Dimensions 107 x 88 x 60 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S4