KNX AQS/TH-UP Touch Indoor Sensor invitation to tender

Indoor sensor for the KNX bus system. Measuring of CO2 content, temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 9 threshold values. Logic links (AND and OR). Integrated PI controller for one- or two-step heating/cooling (temperature) and for one- or two-step ventilation (humidity/CO2). Variable comparators. 224 communication objects. Operating voltage: KNX bus voltage.
With display and touch buttons (keys for target value change, mode change or as bus push-buttons). Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W xH in mm), installation depth approx. 8 mm Base plate dimensions: approx. 71 x 71 (W x H in mm),

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70618, 70619 KNX AQS/TH-UP Touch