KNX TH-UP gl Indoor Sensor invitation to tender

Indoor sensor for the KNX bus system. Measuring of temperature and air humidity (relative, absolute). Calculation of the dew point. Calculation of mixed values. 5 threshold values. Logic links (AND and OR). Integrated PI controller for one- or two-step heating/cooling (temperature) and for one- or two-step ventilation (humidity). Variable comparators. 158 communication objects. Operating voltage: KNX bus voltage.
Wall installation, flush-mounted in equipment socket. Supplied without frame. Housing dimensions: approx. 55 x 55 (W xH in mm), installation depth approx. 8 mm Base plate dimensions: approx. 71 x 71 (W x H in mm),

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70621, 70622 KNX TH-UP gl