KNX S-B4T-UP 230 V AC actuator invitation to tender

Actuator for the KNX bus system. To control shades (shutters, blinds, roller doors) or windows. External or internal setting of the automatic functions possible. Internal automatic functions with blocks, locks and priority stipulations. 8-channel scene memory.
Connection for drive: 1 x 230 V AC fused with microfuse T6.3 A.
Inputs: 4 x binary inputs (for contacts free of potential),1 x temperature sensor.
125 communication objects.
Assembly in built-in socket. Dimensions 50 x 51 x 41 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S-B4T-UP 230 V AC

KNX S-B2-UP 230 V AC actuator invitation to tender

Actuator for the KNX bus system. To control shades (shutters, blinds, roller doors) or windows. External or internal setting of the automatic parameters possible. Internal automatic functions with blocks, locks and priority stipulations. 8-channel scene memory.
Connection for drive: 1 x 230 V AC fused with microfuse T6.3 A.
Inputs: 2 x binary inputs (for contacts free of potential).
88 communication objects.
Assembly in built-in socket. Dimensions 50 x 51 x 41 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S-B2-UP 230 V AC

KNX S-UP 230 V AC actuator invitation to tender

Actuator for the KNX bus system. To control shades (shutters, blinds, roller doors) or windows. External or internal setting of the automatic parameters possible. Internal automatic functions with blocks, locks and priority stipulations. 8-channel scene memory.
Connection for drive: 1 x 230 V AC fused with microfuse T6.3 A.
72 communication objects.
Assembly in built-in socket. Dimensions 50 x 51 x 41 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX S-UP 230 V AC