KNX L Brightness Sensor invitation to tender

Brightness sensor for the KNX bus system. Operating voltage KNX bus voltage. Application with 3 brightness threshold values for daytime, 3 twilight threshold values for night-time, 8 AND logic gates and 8 OR logic gates. 117 communication objects. 
Including combi-mount for wall/mast mounting. Dimensions 96 x 77 x 118 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70119 KNX L