Automation / Sensors

ESYLUX PD-C360i/8 KNX UP360° ceiling-mounted presence detector
recessed-mounted
KNX bus
approx. range Ø 8 m
remotely controlled 

Description:Simple configuration. Inputs for KNX touch sensors for manual override. End user remote control for additional manual dimming/switching (accessory).Mains voltage from KNX bus 29 - 31 V
Bus voltage 29-31 V = (KNX)
Field of detection 360°
Range approx. 8 m in Ø
at an installation height of 3 m to 5 m
Setting options remotely with ETS-Software
temporarily electronically by infrared Mobil-PDi/User and Mobil-PDi/MDi-universal remote controls (order separately)
Permissible ambient temperature 5 °C ...+35 °C
Protection type IP 20
Protection class III
Installation type Ceiling mounting
Housing material UV-stabilised polycarbonate
Approx. dimensions Height 38 mm  
Ø 108 mm
Installation dimension  Installation depth 24 mm
Installation hole size 68 mm
Included in delivery Includes lens mask
Slave input Yes
unit can be configured as a master or slave device
KNX input manual light control
block objects
reset
slave
KNX output presence
status
light value
HVAC
<b>Light channel</b> c1 + c2 switching/dimming
offset (-50 % to +50 %)
Interface <b>KNX</b>
Switch-off delay time disabled/30 sec./1 min./12 hrs
Light measurement mixed light
Light value disabled/approx. 5 - 2000 lux
Orientation light disabled/10 - 50 %
2 values can be selected
Switch-off delay time
orientation light only in controlling modus: continuous lighting/1 min - 250 min
Turn-on delay disabled/2 min - 30 min
Switch-off delay channel 2 10 sec.&ndash;1 hour
Switch-on delay channel 3 disabled/2 min - 30 min
Time setting channel 3 disabled/30 sec./1 min./12 hrs
Switch-off delay time disabled/30 sec./1 min./12 hrs
Power consumption 6 mA
Relative humidity 5 - 93 %
non-condensing
Conformity CE
RoHS

Colour white
similar to RAL 9010 

Manufacturer: ESYLUX 
Order number: EP10427404