                                                                   Revision: 1.0
--------------------------------------------------------------------------------
Package            update-4.1.5_4.2.0-p.cbsa

Version            4.2.0-p

Required version   4.1.5-p

Support models     Server
                   Server Advanced
                   Server 192
                   Virtual Machine

--------------------------------------------------------------------------------
WHAT THIS PACKAGE DOES

 This package updates Evolution system from version 4.1.5-p to version 4.2.0-p.
 This update is generally done manually by the user following the instructions
 in the INSTALLATION section.

--------------------------------------------------------------------------------
NOTES

 Please clear your browser cache after installing this update.
 
--------------------------------------------------------------------------------
LIMITATIONS

 Nothing.

--------------------------------------------------------------------------------
CHANGES IN THIS RELEASE

[4.2.0-p]
- Fix. Hide password menu in editor for evo5.
- Fix. Export html issue when window has no name.
- Fix. Gauge charts are displayed correctly.
- Improvement. Increment subject and content email characteres.
- Improvement. Adding secure flag to connection.
- Fix. Allow speciasl characters in user editor html.
- Improvement. Master slave connection improvement.
- Improvement. In dali module add column device name in topology view.
- Improvement. Allow sub dpt 0 for all dpts.
- Fix. Issue with label temperature in clima elements.

[4.1.5-p]
- Fix. Mouse position correctly in mobile in a scaled visu.
- Fix. Users not visibles can be edit in html.
- Improvement. Add user information in csv export.
- Improvement. Support for rtsp protocol.
- Fix. Massive check and stand by alarms work properlly.
- Fix. Resolved issue scenes with the same name in planner.
- Fix. Task in planner at 00:00 execute properlly.
- Fix. Fixed issue with cameras and host ended with "/"
- Improvement. Automatically close the alarm bar when all alarms have been checked.

[4.1.4-p]
- Install System Update 0.0.1 in Evo5 if it is not installed.
- Fix weekly scheduler automated process points.
- Fix issue on create weekly schedulers on visu, send the right command.
- Show in editor system update version and hardware model version.
- Natural order by name process points and folder in editor.


[4.1.3-p]
- Fixed: With master-slave, the active power of the smart metering is not
  obtained from the database. We only get the data online.
- Fixed: some cases, the client manager service stops. When restarting
  it does not connect correctly with the other services.
- Fixed: Planner issues.
  
[4.1.2-p]

- Implemented custom logic functions to convert datetime to string.
- Implemented new process points to enable/disable weekly schedules.
- Implemented new process points to enable/disable category scenes.
- Implemented new process points to shut down the Evolution server.
- Implemented new property "send on release" in the switch element.
- Improved: The Connection Manager saves the last editor type opened.
- Fixed: Saving ip cams with wrong host causes the web server not to start on
  the next reboot.
- Fixed: The main menu icon on a visualization page is swf instead of png.
- Fixed: Export alarm does not get the separator character.
- Fixed: After export a page, the changes has not been updated.
- Fixed: Order elements by time in Weekly scheduler module.
- Fixed: Scene module is not open when category has strange characters.
- Fixed: Email and Domain validator does not accept some domain formats.
- Fixed: Activate project is done before the web server is stopped.
- Fixed: User cannot load dali module in dali box.
- Fixed: Export project information to PDF and CSV fails.
- Fixed: Scene module hangs.
- Fixed: Advanced chart not working.
- Fixed: Yearly repition does not run correctly in the yearly planner.
- Fixed: Monthly repition does not run correctly in the yearly planner.
- Fixed: GLT object with two datapoints is not working.
- Fixed: Slave infinite loop.
- Fixed: DPT 29 not imported in modbus.
- Fixed: Set Unknown state when master-slave connection is lost and recovery.
- Fixed: Planner does not show scenes.
- Fixed: Smart metering does not work with master-slave.
- Fixed: Rights configuration for scene module does not work properly.
- Fixed: After export HTML page, the changes are not updated. Cache problem.
- Fixed: Estimated cnmsumtion is not calculated correctly in Smart metering
  module.
- Improved: Editor locks while saving.
- Fixed: Services do not restart correctly after activating a project.
- Improved: Improved the scenes load.
- Improved: It is not possible to open a project with errors.
- Improved: Improved ESF import filter. Wildcards '*' and '?' allowed.
- Improved: Show name and Descriptions in ECG Dali module.

--------------------------------------------------------------------------------
INSTALLATION

[EVO5 Systems]

  1. Open a web navigator
  2. Enter the address http://<device_IP>/webmin or http://evo5/webmin
  3. Enter the user and password. If the username and password are not known,
     check the product manual or contact with Futurasmus.
  4. In the side menu, navigate to "Others" -> "Custom commands".
  5. Press the button next to "Evolution Package to upload" and search the
     update package file.
  6. Press the "Evolution Package Installer" button. Installation will begin.
     - The installation process can take several minutes. Do not close the
       browser tab or your Evolution system until you have finished.
     - If the system does not have the required previous version installed,
       the installation will be canceled.
     - If the system does not meet the conditions in the LIMITATIONS section,
       the following message will appear and the installation will be canceled.

       ***************************************************
       **                                               **
       **                                               **
       **       YOUR HARDWARE IS NOT COMPATIBLE!        **
       **                                               **
       **                                               **
       ***************************************************

  7. When the installation process is complete, it will display the result.
  8. In the side menu, navigate to "System" -> "Bootup and Shutdown".
  9. At the bottom of the page that opens, press the "Reboot System" button.
 10. Press "Reboot System" button again. The system will restart.

[Other systems]

 1. Open a web navigator
 2. Enter the address http://<device_IP>:8181/upload.php
 3. Enter the user and password. If the username and password are not known,
    check the product manual or contact with Futurasmus.
 4. Press "Select file" button and search the update package file.
 5. Press "INSTALL" button. Installation will begin.
    - The installation process can take several minutes. Do not close the
      browser tab or your Evolution system until you have finished.
    - If the system does not have the required previous version installed,
      the installation will be canceled.
    - If the system does not meet the conditions in the LIMITATIONS section,
      the following message will appear and the installation will be canceled.

      ***************************************************
      **                                               **
      **                                               **
      **       YOUR HARDWARE IS NOT COMPATIBLE!        **
      **                                               **
      **                                               **
      ***************************************************

 6. When the installation process is complete, it will display the result in
    the text field of the web page. After a few seconds the system will
    restart.

