KNX RW sl Rain/Wind Sensor invitation to tender

Combi-sensor for the KNX bus system. Detection of precipitation and wind speed. Operating voltage 12…40 V DC / 12...28 V AC. Application with 4 wind threshold values, 1 rain switching output, 8 multi-functional calculator modules, 8 AND logic gates and 8 OR logic gates. 182 communication objects. 
For wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 70162 KNX RW sl