P03/3-Modbus-GPS weather station invitation to tender

Weather station with Modbus data output, RS485 2-wire, Modbus RTU protocol. Recording of brightness (3 sensors), wind speed (electronic measurement), precipitation (heated sensor) and temperature. With GPS receiver (output of UTC, position and sun's position). Including combi-mount for wall/mast mounting
Dimensions 96 x 77 x 118 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 30147 P03/3-Modbus-GPS

P03/3-Modbus weather station invitation to tender

Weather station with Modbus data output, RS485 2-wire, Modbus RTU protocol. Recording of brightness (3 sensors), wind speed (electronic measurement), precipitation (heated sensor) and temperature. Including combi-mount for wall/mast mounting
Dimensions 96 x 77 x 118 (W x H x D in mm)

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: 30146 P03/3-Modbus